## Seated Workstation Specifications

|  |
| --- |
| Illustration of Seated Workstation Dimensions |
| F:\SeatedWSLayout.jpg |

### Seated Workstation Dimensions

|  |  |  |
| --- | --- | --- |
| **Criteria** | **Dimension** | **Description** |
| **A.  Worksurface height**  | Adjustable Worksurface | Fixed Height Worksurface (with chair/ footrest) | Distance from the floor to placement of hands on the work surface. **NOTE: This may not be the actual worksurface height - it reflects the hand work height based on size of the object**. |
| * Precision work
 | 26” to 36” | 34” |
| * Light assembly
 | 22” to 32” | 29” |
| * Manual work
 | 20” to 28” | 26” |
| **B**.**Work surface thickness** | Fixed: 46” | Allows for thigh clearance. |
| **C.  Screen height** | Maximum of 2”, adjustable: 44” to 50” | Distance from floor to top of screen. |
| **D.  Knee space - width** | Minimum of 20” | Side-to-side clearance for legs. |
| **E.  Knee space - front to back** | Minimum of 16" | Allows for knee clearance. |
| **F.  Thigh clearance** | Minimum of 8” | Seatpan top to undersurface of the worksurface. |
| **G.  Distance to work** | Up to 4” | Front of worksurface to hand work position. |
| **H. Foot space depth** | Minimum of 4” | Allows for foot clearance. |
| **I.   Distance for toe clearance** | Minimum of 20" | Allows for foot clearance with legs extended. |
| **J.  Foot space**  | Minimum of 4” | Allows for foot clearance. |